Serial Port | Operation Mode | Listen Port | Trust Type | Max Connection | Connection Control | Connection Idle Timeout | Alive Check Timeout | Enable | Action
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
SPort-0 |  | (1~65535) |  |  |  | (0-60)min | (0-60)min |  |
Serial Port | Data Buffer Length | Delimiter Character 1 | Delimiter Character 2 | Data Timeout Transmit
--- | --- | --- | --- | ---
SPort-0 | (0~1024) | (Hex) Enable | (Hex) Enable | (0~1000ms)
ID | To Remote Host | Remote Port | Serial Port | Definition Enable | Action
--- | --- | --- | --- | --- | ---
1 |  |  |  |  |
2 |  |  |  |  |
3 |  |  |  |  |
4 |  |  |  |  |
ID | Remote Host | Remote Port | Serial Port | Definition Enable | Action
--- | --- | --- | --- | --- | ---
1 | - |  |  |  |
2 | - |  |  |  |
3 | - |  |  |  |
4 | - |  |  |  |
ID | Host | Serial Port | Definition Enable | Action
--- | --- | --- | --- | ---
1 | - | SPort-0 |  |
2 | - | SPort-0 |  |
3 | - | SPort-0 |  |
4 | - | SPort-0 |  |
5 | - | SPort-0 |  |
6 | - | SPort-0 |  |
7 | - | SPort-0 |  |
8 | - | SPort-0 |  |