Item | Setting
--- | ---
Tunnel | Enable
Tunnel Name |
Interface |
Tunnel Scenario |
Hub and Spoke |
Operation Mode |
Encapsulation Protocol |
Encapsulation Protocol |
Keep alive | Enable Interval(seconds)
Item | Setting
--- | ---
Local Subnet List |
ID | Subnet IP Address | Subnet Mask | Actions
--- | --- | --- | ---
1 |  |  |
Redirect Traffic | Enable
Full Tunnel | Enable
Remote Subnet List |
ID | Subnet IP Address | Subnet Mask | Actions
--- | --- | --- | ---
1 |  |  |
Remote Gateway | (IP Address/FQDN)
Item | Setting
--- | ---
Local Subnet |
Local Netmask |
Remote Subnet |
Remote Netmask |
Remote Gateway | (IP Address/FQDN)
Item | Setting
--- | ---
Key Management | Show Local Certificate: Remote Certificate:
Local ID | Type: ID: (Optional)
Remote ID | Type: ID:
Item | Setting
--- | ---
IKE Version |
Negotiation Mode |
X-Auth | (Optional) User Name : Password : Show
Dead Peer Detection (DPD) | Enable Timeout : (seconds)Delay : (seconds)
Phase1 Key Life Time | (seconds)(Max. 86400)
ID | Encryption | Authentication | DH Group | Definition
--- | --- | --- | --- | ---
1 |  |  |  | Enable
2 |  |  |  | Enable
3 |  |  |  | Enable
4 |  |  |  | Enable
Item | Setting
--- | ---
Phase2 Key Life Time | (seconds)(Max. 86400)
ID | Encryption | Authentication | PFS Group | Definition
--- | --- | --- | --- | ---
1 |  |  |  | Enable
2 |  |  | Enable
3 |  |  | Enable
4 |  |  | Enable
Item | Setting
--- | ---
Outbound SPI | 0x
Inbound SPI | 0x
Encryption |
Authentication |