Item | Setting
--- | ---
IPSec | Enable
NetBIOS over IPSec | Enable
NAT Traversal | Enable
Max. Concurrent IPSec Tunnels | 16
Dynamic VPN List
ID | Tunnel Name | Interface | Tunnel Scenario | Remote Gateway | Remote Subnet | Status | Enable | Actions
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 | Dynamic IPSec1 |  | Dynamic VPN | Any | Any |  |  |
2 |  |  |  |  |  |  |  |
Dynamic VPN List
ID | Tunnel Name | Interface | Connected Client | Enable | Actions
--- | --- | --- | --- | --- | ---
IPSec Tunnel List
ID | Tunnel Name | Interface | Tunnel Scenario | Remote Gateway | Remote Subnet | Status | Enable | Actions
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 | IPSec #1 |  | Site to Site | 192.168.1.2 | 192.168.1.1/255.255.255.0 |  |  | Select
1 | *VPN is used by L2TP over IPsec.
*Dynamic IP VPN is used by L2TP over IPsec.