Op. Band | ID | WiFi Enable | Op. Mode | SSID | Channel | WiFi System | Auth.&Security | MAC Address | Action
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
2.4G | VAP-1 |  | AP Router | NetComm_2.4GHz | Auto | b/g/n Mixed | WPA2-PSK(AES) | 00:50:18:00:00:08 | 5 3
2.4G | VAP-2 |  | AP Router | default | Auto | b/g/n Mixed | Auto(None) | 02:50:18:00:00:08 | 2 0
2.4G | VAP-3 |  | AP Router | default | Auto | b/g/n Mixed | Auto(None) | 02:50:18:01:00:08 | 2 0
2.4G | VAP-4 |  | AP Router | default | Auto | b/g/n Mixed | Auto(None) | 02:50:18:02:00:08 | 2 0
2.4G | VAP-5 |  | AP Router | default | Auto | b/g/n Mixed | Auto(None) | 02:50:18:03:00:08 | 2 0
2.4G | VAP-6 |  | AP Router | default | Auto | b/g/n Mixed | Auto(None) | 02:50:18:04:00:08 | 2 0
2.4G | VAP-7 |  | AP Router | default | Auto | b/g/n Mixed | Auto(None) | 02:50:18:05:00:08 | 2 0
2.4G | VAP-8 |  | AP Router | Guest | Auto | b/g/n Mixed | Auto(None) | 02:50:18:06:00:08 | 2 0
0
Op. Band | ID | WiFi Enable | Op. Mode | SSID | Channel | WiFi System | Auth.&Security | MAC Address | Action
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
5G | VAP-1 |  | AP Router | NetComm_5GHz | Auto | a/n/ac Mixed | WPA2-PSK(AES) | 00:50:18:00:06:08 | 5 3
5G | VAP-2 |  | AP Router | default | Auto | a/n/ac Mixed | Open(None) | 02:50:18:00:06:08 | 0 0
5G | VAP-3 |  | AP Router | default | Auto | a/n/ac Mixed | Open(None) | 02:50:18:01:06:08 | 0 0
5G | VAP-4 |  | AP Router | default | Auto | a/n/ac Mixed | Open(None) | 02:50:18:02:06:08 | 0 0
5G | VAP-5 |  | AP Router | default | Auto | a/n/ac Mixed | Open(None) | 02:50:18:03:06:08 | 0 0
5G | VAP-6 |  | AP Router | default | Auto | a/n/ac Mixed | Open(None) | 02:50:18:04:06:08 | 0 0
5G | VAP-7 |  | AP Router | default | Auto | a/n/ac Mixed | Open(None) | 02:50:18:05:06:08 | 0 0
5G | VAP-8 |  | AP Router | Guest_5GHz | Auto | a/n/ac Mixed | Open(None) | 02:50:18:06:06:08 | 0 0
0
SSID | BSSID | Channel | Security | RSSI0 | RSSI1 | Rate | Action
--- | --- | --- | --- | --- | --- | --- | ---
default |  | 11 | Open(None) | 0 | 0 | 0 |
SSID | BSSID | Channel | Security | RSSI0 | RSSI1 | Rate | Action
--- | --- | --- | --- | --- | --- | --- | ---
default |  | 36 | Open(None) | 0 | 0 | 0 |
SSID | Remote AP MAC | Channel | Security | RSSI0 | RSSI1 | Action
--- | --- | --- | --- | --- | --- | ---
NetComm_2.4GHz |  | Auto | WPA2-PSK(AES) | 0 0 0 0 | 0 0 0 0 |
SSID | Remote AP MAC | Channel | Security | RSSI0 | RSSI1 | Action
--- | --- | --- | --- | --- | --- | ---
NetComm_5GHz |  | Auto | WPA2-PSK(AES) | 0 0 0 0 | 0 0 0 0 |
Authentication Frame | Association Request Frame | Re-association Request Frame | Probe Request Frame | Disassociation Frame | Deauthentication Frame | EAP Request Frame | Malicious Data Frame | Action
--- | --- | --- | --- | --- | --- | --- | --- | ---
0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
Authentication Frame | Association Request Frame | Re-association Request Frame | Probe Request Frame | Disassociation Frame | Deauthentication Frame | EAP Request Frame | Malicious Data Frame | Action
--- | --- | --- | --- | --- | --- | --- | --- | ---
0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
Op. Band | ID | Received Packets | Transmitted Packets | Action
--- | --- | --- | --- | ---
2.4G | VAP-1 | 0 | 0 |
2.4G | VAP-2 | 0 | 0 |
2.4G | VAP-3 | 0 | 0 |
2.4G | VAP-4 | 0 | 0 |
2.4G | VAP-5 | 0 | 0 |
2.4G | VAP-6 | 0 | 0 |
2.4G | VAP-7 | 0 | 0 |
2.4G | VAP-8 | 0 | 0 |
Op. Band | ID | Received Packets | Transmitted Packets | Action
--- | --- | --- | --- | ---
5G | VAP-1 | 0 | 0 |
5G | VAP-2 | 0 | 0 |
5G | VAP-3 | 0 | 0 |
5G | VAP-4 | 0 | 0 |
5G | VAP-5 | 0 | 0 |
5G | VAP-6 | 0 | 0 |
5G | VAP-7 | 0 | 0 |
5G | VAP-8 | 0 | 0 |