Item | Setting
--- | ---
IPv4 Static Routing | Enable
IPv6 Static Routing | Enable
IPv4 Static Routing Rule List
ID | Destination IP | Subnet Mask | Gateway IP | Interface | Metric | Enable | Actions
--- | --- | --- | --- | --- | --- | --- | ---
1 | 192.168.1.1 | 255.255.255.0 | 192.168.1.2 | Auto | 1 |  | Select
IPv6 Static Routing Rule List
ID | Destination IP | Prefix Length | Gateway IP | Interface | Metric | Enable | Actions
--- | --- | --- | --- | --- | --- | --- | ---
1 | 192.168.1.1 | 30 | 192.168.1.2 | WAN-1 | 5 |  | Select