> Statistics -- xDSL

> Mode: | VDSL2
> Traffic Type: | PTM
> Status: | Up
> Link Power State: | L0
> | Downstream | Upstream
> Line Coding(Trellis): | On | Off
> SNR Margin (0.1 dB): | 121 | 79
> Attenuation (0.1 dB): | 268 | 0
> Output Power (0.1 dBm): | 143 | 89
> Attainable Rate (Kbps): | 112273 | 22213
> | Path 0 |  | Path 1 |
> | Downstream | Upstream | Downstream | Upstream
> Rate (Kbps): | 79940 | 20007 | 0 | 0
> B (# of bytes in Mux Data Frame): | 63 | 79 | 0 | 0
> M (# of Mux Data Frames in an RS codeword): | 1 | 1 | 0 | 0
> T (# of Mux Data Frames in an OH sub-frame): | 64 | 64 | 0 | 0
> R (# of redundancy bytes in the RS codeword): | 16 | 2 | 0 | 0
> S (# of data symbols over which the RS code word spans): | 0.0255 | 0.0255 | 0.0255 | 0.0255
> L (# of bits transmitted in each data symbol): | 25128 | 5160 | 25128 | 5160
> D (interleaver depth): | 1241 | 1 | 0 | 0
> I (interleaver block size in bytes): | 80 | 41 | 0 | 0
> N (RS codeword size): | 80 | 82 | 0 | 0
> Delay (msec): | 8 | 0 | 0 | 0
> INP (DMT symbol): | 3.00 | 0.00 | 0.00 | 0.00
> OH Frames: | 16306297 | 3242104 | 0 | 0
> OH Frame Errors: | 0 | 125 | 0 | 0
> RS Words: | 586489483 | 117955007 | 0 | 0
> RS Correctable Errors: | 65 | 48 | 0 | 0
> RS Uncorrectable Errors: | 0 | 0 | 0 | 0
> HEC Errors: | 1076 | 0 | 0 | 0
> OCD Errors: | 0 | 0 | 0 | 0
> LCD Errors: | 0 | 0 | 0 | 0
> Total Cells: | 576491094 | 0 | 0 | 0
> Data Cells: | 9191 | 0 | 0 | 0
> Bit Errors: | 0 | 0 | 0 | 0
> Total ES: | 9 | 125
> Total SES: | 10 | 0
> Total UAS: | 86858 | 86840