> ATM PVC Configuration
> This screen allows you to configure a ATM PVC.

> VPI: | [0-255]
> VCI: | [32-65535]

> Select DSL Latency
> Path0 (Fast)
> Path1 (Interleaved)

> Select DSL Link Type (EoA is for PPPoE, IPoE, and Bridge.)
> EoA
> PPPoA
> IPoA

> Encapsulation Mode: |

> Service Category: |

> Peak Cell Rate: | [cells/s]

> Sustainable Cell Rate: | [cells/s]
> Maximum Burst Size: | [cells]

> Minimum Cell Rate: | [cells/s] (-1 indicates no shaping)

> Default Queue Drop Algorithm

> DT (Drop Tail)

> RED (Random Early Detection)
> Minimum Threshold: | [1-100]% of queue size
> Maximum Threshold: | [1-100]% of queue size

> WRED (Weighted RED)
> Low Class Min Threshold: | [1-100]% of queue size
> Low Class Max Threshold: | [1-100]% of queue size
> High Class Min Threshold: | [1-100]% of queue size
> High Class Max Threshold: | [1-100]% of queue size

> VC WRR Weight: | [1-63]
> VC Precedence:

> Note: VC scheduling will be SP among unequal precedence VC's and WRR among equal precedence VC's.
> For single queue VC, the default queue precedence and weight will be used for arbitration.
> For multi-queue VC, its VC precedence and weight will be used for arbitration.