> WAN Service Configuration

> Select WAN service type:
> PPP over Ethernet (PPPoE)
> IP over Ethernet
> Bridging
> Allow as IGMP Multicast Source
> Allow as MLD Multicast Source

> Enter Service Description: |

> For tagged service, enter valid 802.1P Priority and 802.1Q VLAN ID.
> For untagged service, set -1 to both 802.1P Priority and 802.1Q VLAN ID.
> Enter 802.1P Priority [0-7]: |
> Enter 802.1Q VLAN ID [0-4094]: |
> Select VLAN TPID: |

> Internet Protocol Selection: