> IPv6 LAN Auto Configuration
> Note: Stateful DHCPv6 is supported based on the assumption of prefix length less than 64. Interface ID does NOT support ZERO COMPRESSION "::". Please enter the complete information. For example: Please enter "0:0:0:2" instead of "::2".

> Static LAN IPv6 Address Configuration
> Interface Address (prefix length is required): |

> IPv6 LAN Applications

> | Enable DHCPv6 Server

> Stateless
> Stateful
> Start interface ID: |
> End interface ID: |
> Leased Time (hour): |

> | Enable RADVD

> Enable ULA Prefix Advertisement
> Randomly Generate
> Statically Configure

> Prefix: |

> Preferred Life Time (Seconds): |

> Valid Life Time (Seconds): |

> Enable MLD Snooping

> Standard Mode
> Blocking Mode
> Enable MLD LAN to LAN Multicast: |
> (LAN to LAN Multicast is enabled until the first WAN service is connected, regardless of this setting.)