Advanced
This page allows you to configure the Physical Wireless interfaces.

Wireless Interface: |  |

Country: |  | Current: AU |
Regulatory Revision: |  | Current: 0

Interface: |  |
802.11 Band: |  |
Channel Specification: |  |
802.11 n-mode: |  |
Bandwidth: |  | Current: 80MHz
Control Sideband |  |
NPHY Rate: |  |
NPHY TxChains: |  |
NPHY RxChains: |  |
54g™ Mode: |  |
802.11n Protection: |  |
VLAN Priority Support: |  |
Rate: |  |
Basic Rate Set: |  |
Multicast Rate: |  |

Regulatory Mode: |  |
DFS Preferred Channel List: |  |
TPC Mitigation (db): |  |

OBSS Coexistence: |  |

Fragmentation Threshold: |  |
RTS Threshold: |  |
DTIM Interval: |  |
Beacon Interval: |  |
Beacon Rotation: |  |
Preamble Type: |  |
Max Associations Limit: |  |

XPress™ Technology: |  |

SW Probe Response: |  |

Beamforming transmission (BFR): |  |
Beamforming reception (BFE): |  |
MU-MIMO TX: |  |

RIFS Mode Advertisement: |  |

WMM Support: |  |
No-Acknowledgement: |  |
APSD Support: |  |
EDCA AP Parameters: |  | CWmin | CWmax | AIFSN | TXOP(b) Limit (usec) | TXOP(a/g) Limit (usec) | Admission Control | Discard Oldest First
AC_BE |  |  |  |  |  |  |  |
AC_BK |  |  |  |  |  |  |  |
AC_VI |  |  |  |  |  |  |  |
AC_VO |  |  |  |  |  |  |  |
EDCA STA Parameters:
AC_BE |  |  |  |  |  |  |  |
AC_BK |  |  |  |  |  |  |  |
AC_VI |  |  |  |  |  |  |  |
AC_VO |  |  |  |  |  |  |  |

Mode: |  |
Network: |  |
URE Mode: |  |
Band Steering: |  |

STA Retry Time(sec): |  |  |

Bridges: |  | Peer MAC Address |  | Link Status
Bridge Restriction: |  |
Bridge Link Detection Interval: |  |