> WAN IP Settings
> Enter information provided to you by your ISP to configure the WAN IP settings.
> Notice: If "Obtain an IP address automatically" is chosen, DHCP will be enabled for PVC in IPoE mode.
> If "Use the following Static IP address" is chosen, enter the WAN IP address, subnet mask and interface gateway.

> Obtain an IP address automatically
> Option 60 Vendor ID: |
> Option 61 IAID: |  |  | (8 hexadecimal digits)
> Option 61 DUID: |  |  | (16 hexadecimal digits)
> Option 77 User ID: |
> Option 125: | Disable | Enable
> Option 50 Request IP Address: |
> Option 51 Request Leased Time: |
> Option 54 Request Server Address: |
> Use the following Static IP address:
> WAN IP Address: |
> WAN Subnet Mask: |
> WAN gateway IP Address: |
> Primary DNS server: |
> Secondary DNS server: |

> Enter information provided to you by your ISP to configure the WAN IPv6 settings.
> Notice:
> If "Obtain an IPv6 address automatically" is chosen, DHCPv6 Client will be enabled on this WAN interface.
> If "Use the following Static IPv6 address" is chosen, enter the static WAN IPv6 address. If the address prefix length is not specified, it will be default to /64.

> Obtain an IPv6 address automatically
> Dhcpv6 Address Assignment (IANA)
> Dhcpv6 Prefix Delegation (IAPD)
> Use the following Static IPv6 address:
> WAN IPv6 Address/Prefix Length: |

> Specify the Next-Hop IPv6 address for this WAN interface.
> Notice: This address can be either a link local or a global unicast IPv6 address.

> WAN Next-Hop IPv6 Address: |