> Device Info

> Build Timestamp: | 20230509_1145
> NL20MESH.NC.UR-R6B021.EN
> Bootloader (CFE) Version: | 1.0.38-163.243
> Voice Service Version: | Voice
> Uptime: | 0D 4H 51M 7S

> This information reflects the current status of your WAN connection.

> LAN IPv4 Address: | 192.168.20.1
> Default Gateway:
> Primary DNS Server: | 202.96.128.86, 240e:1f:1::1
> Secondary DNS Server: | 202.96.134.133, 240e:1f:1::33