> Wide Area Network (WAN) Service Setup
> Choose Add, Remove or Edit to configure a WAN service over a selected interface.

> Interface | Description | Type | Vlan8021p | VlanMuxId | VlanTpid | Igmp Proxy | Igmp Source | NAT | Firewall | IPv6 | Mld Proxy | Mld Source | Remove | Edit |
> eth4.1 | ETH WAN | IPoE | N/A | N/A | N/A | Disabled | Disabled | Enabled | Enabled | Enabled | Disabled | Disabled |  |  |
> ptm0.2 | VDSL | IPoE | N/A | N/A | N/A | Disabled | Disabled | Enabled | Enabled | Enabled | Disabled | Disabled |  |  |