> IPv6 LAN Auto Configuration
> Note:
> 1:Stateful DHCPv6 is supported based on the assumption of prefix length less than 64. Interface ID does NOT support ZERO COMPRESSION "::". Please enter the complete information. For exampe: Please enter "0:0:0:2" instead of "::2".
> 2: Unique local address must start with "fd". The prefix and the address must be in same network and the prefix lenght must be 64.

> Enable ULA Prefix Advertisement

> Randomly Generate
> Statically Configure

> Interface Address (prefix length is required): | (e.g: fd80::/64)

> Prefix: |

> Preferred Life Time (hour): |

> Valid Life Time (hour): |

> IPv6 LAN Applications

> | Enable DHCPv6 Server

> Stateless
> Stateful
> Start interface ID: |
> End interface ID: |
> Leased Time (hour): |

> | Enable RADVD

> Enable MLD Snooping

> Standard Mode
> Blocking Mode
> Enable MLD LAN to LAN Multicast: |
> (LAN to LAN Multicast is enabled until the first WAN service is connected, regardless of this setting.)

> Enable Relay

> DHCPv6 Server IP Address: |
> Selected WAN Interface |
> Hop limit: |