> Wireless -- Advanced
> This page allows you to configure advanced features of the wireless LAN interface. You can select a particular channel on which to operate, force the transmission rate to a particular speed, set the fragmentation threshold, set the RTS threshold, set the wakeup interval for clients in power-save mode, set the beacon interval for the access point, set XPress mode and set whether short or long preambles are used.
> Click "Apply/Save" to configure the advanced wireless options.

> Band:
> Channel: |  | Current Channel:
> Auto Channel Timer(min) |

> 802.11n/EWC: |

> Bandwidth: |  | Current Bandwidth:
> Control Sideband: |  | Current Control Sideband:
> 802.11n Rate: |
> 802.11n Protection: |
> Support 802.11n Client Only: |
> RIFS Advertisement: |
> OBSS Coexistence: |
> RX Chain Power Save: |  | Power Save status: |
> RX Chain Power Save Quiet Time: |
> RX Chain Power Save PPS: |

> 54g™ Rate: |
> Multicast Rate: |
> Basic Rate: |
> Fragmentation Threshold: |
> RTS Threshold: |
> DTIM Interval: |
> Beacon Interval: |
> Global Max Clients: |
> XPress™ Technology: |

> 54g™ Mode: |
> 54g™ Protection: |

> Regulatory Mode: |
> Pre-Network Radar Check: |
> In-Network Radar Check: |
> TPC Mitigation(db): |

> Afterburner Technology: |  | (Disable WMM for Selection)

> Preamble Type: |

> Transmit Power: |

> WMM(Wi-Fi Multimedia): |  |

> WMM No Acknowledgement: |

> WMM APSD: |

> Iperf Support: |
> Video Error Correction: |

> Wireless Mode: |
> URE: |
> URE Mode: |
> STA Retry Time(sec): |

> Beamforming Transmission (BFR): |
> Beamforming Reception (BFE): |

> Band Steering: |
> BSD Role Config: | IP Addr | Port Number
> Helper Addr & Port: |  |
> Primary Addr & Port |  |

> Enable Traffic Scheduler: |
> Enable EBOS Scheduling: |
> Airtime Fairness: |

> Stalled Link Detection Treshold: |
> Packet Saving Retry Limit: |

> ACS Mode: |
> DFS Channel Selection: |
> CI Scan Interval: |
> CI Scan Timeout: |
> Scan Result Expiry: |
> Tx IDLE Frame Rate: |
> Chan Dwell Time: |
> Chan FLOP Period: |
> Sample Period: |
> Sample Count: |
> Non-TCP Stream TxFail Threshold: |
> TCP Stream TxFail Threshold: |
> DFS Reentry Window Settings: | Seconds | Threshold
> Immediate Reentry: |  |
> Deferred Reentry: |  |
> Channel Active: |  |