> Wireless -- Security
> This page allows you to configure security features of the wireless LAN interface.
> You may setup configuration manually
> OR
> through WiFi Protcted Setup(WPS)
> Note: When both STA PIN and Authorized MAC are empty, PBC is used. If Hide Access Point enabled or Mac filter list is empty with "allow" chosen, WPS2 will be disabled

> WPS Setup

> Enable WPS |

> <%ejGetWl(wlScanResult)%>

> Enable Build-In Registrar |

> Add Client (This feature is available only when WPA-PSK(WPS1), WPA2 PSK or OPEN mode is configured)

> | Push-Button Enter STA PIN Use AP PIN |

> |  | Help

> Set Authorized Station MAC

> |  | Help

> Set WPS AP Mode |

> Device PIN |  | Help

> Manual Setup AP
> You can set the network authentication method, selecting data encryption,
> specify whether a network key is required to authenticate to this wireless network and specify the encryption strength.
> Click "Apply/Save" when done.

> Select SSID: |
> Network Authentication: |

> Protected Management Frames: |

> WPA2 Preauthentication: |

> Network Re-auth Interval: |

> WPA/WAPI passphrase: |  |  | Click here to display

> WPA Group Rekey Interval: |

> RADIUS Server IP Address: |
> RADIUS Port: |
> RADIUS Key: |

> WPA/WAPI Encryption: |

> WEP Encryption: |

> Encryption Strength: |
> Current Network Key: |
> Network Key 1: |
> Network Key 2: |
> Network Key 3: |
> Network Key 4: |
> | Enter 13 ASCII characters or 26 hexadecimal digits for 128-bit encryption keys
> | Enter 5 ASCII characters or 10 hexadecimal digits for 64-bit encryption keys

> WAPI Certificate

> Certificate Status: | <%ejGetWl(wlWapiApCertStatus)%> |
> ASU Certificate File: |
> User Certificate File: |