> NAT -- Port Triggering Setup
> Some applications require that specific ports in the Router's firewall be opened for access by the remote parties. Port Triggering dynamically opens the 'Open ports' in the firewall when an application on the LAN initiates a TCP/UDP connection to a remote party using the 'Triggering Ports'. The Router allows the remote party from the WAN side to establish new connections to the application on the LAN side using the 'Open Ports'. A maximum of 32 entries can be configured.

> Application Name | Trigger | Open | WAN Interface | Remove
> Protocol | Port Range | Protocol | Port Range
> Start | End | Start | End