> Local Area Network (LAN) Setup
> Configure the Broadband Router IP Address and Subnet Mask for LAN interface. GroupName

> IP Address: |
> Subnet Mask: |

> Enable IGMP Snooping

> Standard Mode
> Blocking Mode
> Enable IGMP LAN to LAN Multicast: |
> LAN2LAN multicast setting takes effect only when WAN service is up.
> LAN2LAN multicast is always enabled when WAN service is down regardless of this setting.

> Enable LAN side firewall

> Disable DHCP Server
> Enable DHCP Server
> Start IP Address: |
> End IP Address: |
> Primary DNS server: |
> Secondary DNS server: |
> Leased Time (hour): |

> DHCP advanced settings

> Static IP Lease List: (A maximum 32 entries can be configured)

>   MAC Address | IP Address | Remove

> Enable DHCP Server Relay
> DHCP Server IP Address: |

> Configure the second IP Address and Subnet Mask for LAN interface

> IP Address: |
> Subnet Mask: |