> NAT -- Virtual Servers Setup
> Virtual Server allows you to direct incoming traffic from the WAN interface (identified by its Protocol and External port) to the Internal server with a private IP address on the LAN interface. The Internal port is required only if the external port needs to be converted to a different port number used by the server on the LAN side. A maximum of 64 entries can be configured.
> Note: An IPv4 address is not editable if the IPv4 NAT function is turned off.
> Note: An IPv6 address is not editable if the IPv6 function of the interface is turned off.

> Server Name | External Port Start | External Port End | Protocol | Internal Port Start | Internal Port End | Server IPv4 Address | Server IPv6 Address | WAN Interface | LAN Loopback | Remove