> Routing -- RIP Configuration
> NOTE: If selected interface has NAT enabled, only Passive mode is allowed.
> To activate RIP for the WAN Interface, select the desired RIP version and operation and place a check in the 'Enabled' checkbox. To stop RIP on the WAN Interface, uncheck the 'Enabled' checkbox. Click the 'Apply/Save' button to star/stop RIP and save the configuration.

> Interface | Version | Operation | Enabled
> eth4.1 |  |  |
> ptm0.2 |  |  |