> QoS Queue Setup
> In PTM mode, maximum 8 queues can be configured.
> For each Ethernet interface, maximum 8 queues can be configured.
> For each Ethernet WAN interface, maximum 8 queues can be configured.
> To add a queue, click the Add button.
> To remove queues, check their remove-checkboxes, then click the Remove button.
> The Enable button will scan through every queues in the table. Queues with enable-checkbox checked will be enabled. Queues with enable-checkbox un-checked will be disabled.
> The enable-checkbox also shows status of the queue after page reload.

> Name | Key | Interface | Qid | Prec/Alg/Wght | PtmPrio | DropAlg/ LoMin/LoMax/HiMin/HiMax | ShapingRate (bps) | MinBitRate(bps) | BurstSize(bytes) | Enable | Remove
> LAN Q8 | 65 | eth0 | 8 | 1/SP |  | DT |  |  |  |  |
> LAN Q7 | 66 | eth0 | 7 | 2/SP |  | DT |  |  |  |  |
> LAN Q6 | 67 | eth0 | 6 | 3/SP |  | DT |  |  |  |  |
> LAN Q5 | 68 | eth0 | 5 | 4/SP |  | DT |  |  |  |  |
> LAN Q4 | 69 | eth0 | 4 | 5/SP |  | DT |  |  |  |  |
> LAN Q3 | 70 | eth0 | 3 | 6/SP |  | DT |  |  |  |  |
> LAN Q2 | 71 | eth0 | 2 | 7/SP |  | DT |  |  |  |  |
> LAN Q1 | 72 | eth0 | 1 | 8/SP |  | DT |  |  |  |  |
> LAN Q8 | 73 | eth1 | 8 | 1/SP |  | DT |  |  |  |  |
> LAN Q7 | 74 | eth1 | 7 | 2/SP |  | DT |  |  |  |  |
> LAN Q6 | 75 | eth1 | 6 | 3/SP |  | DT |  |  |  |  |
> LAN Q5 | 76 | eth1 | 5 | 4/SP |  | DT |  |  |  |  |
> LAN Q4 | 77 | eth1 | 4 | 5/SP |  | DT |  |  |  |  |
> LAN Q3 | 78 | eth1 | 3 | 6/SP |  | DT |  |  |  |  |
> LAN Q2 | 79 | eth1 | 2 | 7/SP |  | DT |  |  |  |  |
> LAN Q1 | 80 | eth1 | 1 | 8/SP |  | DT |  |  |  |  |
> LAN Q8 | 81 | eth2 | 8 | 1/SP |  | DT |  |  |  |  |
> LAN Q7 | 82 | eth2 | 7 | 2/SP |  | DT |  |  |  |  |
> LAN Q6 | 83 | eth2 | 6 | 3/SP |  | DT |  |  |  |  |
> LAN Q5 | 84 | eth2 | 5 | 4/SP |  | DT |  |  |  |  |
> LAN Q4 | 85 | eth2 | 4 | 5/SP |  | DT |  |  |  |  |
> LAN Q3 | 86 | eth2 | 3 | 6/SP |  | DT |  |  |  |  |
> LAN Q2 | 87 | eth2 | 2 | 7/SP |  | DT |  |  |  |  |
> LAN Q1 | 88 | eth2 | 1 | 8/SP |  | DT |  |  |  |  |
> LAN Q8 | 89 | eth3 | 8 | 1/SP |  | DT |  |  |  |  |
> LAN Q7 | 90 | eth3 | 7 | 2/SP |  | DT |  |  |  |  |
> LAN Q6 | 91 | eth3 | 6 | 3/SP |  | DT |  |  |  |  |
> LAN Q5 | 92 | eth3 | 5 | 4/SP |  | DT |  |  |  |  |
> LAN Q4 | 93 | eth3 | 4 | 5/SP |  | DT |  |  |  |  |
> LAN Q3 | 94 | eth3 | 3 | 6/SP |  | DT |  |  |  |  |
> LAN Q2 | 95 | eth3 | 2 | 7/SP |  | DT |  |  |  |  |
> LAN Q1 | 96 | eth3 | 1 | 8/SP |  | DT |  |  |  |  |
> Default Queue | 105 | ptm0 | 1 | 8/WRR/1 | Low | DT |  |  |  |  |
> WAN Q8 | 106 | eth4 | 8 | 1/SP |  | DT |  |  |  |  |
> WAN Q7 | 107 | eth4 | 7 | 2/SP |  | DT |  |  |  |  |
> WAN Q6 | 108 | eth4 | 6 | 3/SP |  | DT |  |  |  |  |
> WAN Q5 | 109 | eth4 | 5 | 4/SP |  | DT |  |  |  |  |
> WAN Q4 | 110 | eth4 | 4 | 5/SP |  | DT |  |  |  |  |
> WAN Q3 | 111 | eth4 | 3 | 6/SP |  | DT |  |  |  |  |
> WAN Q2 | 112 | eth4 | 2 | 7/SP |  | DT |  |  |  |  |
> WAN Q1 | 113 | eth4 | 1 | 8/SP |  | DT |  |  |  |  |