> Interface grouping Configuration
> To create a new interface group:
> 1. Enter the Group name and the group name must be unique and select either 2. (dynamic) or 3. (static) below:
> 2. If you like to automatically add LAN clients to a WAN Interface in the new group add the DHCP vendor ID string. By configuring a DHCP vendor ID string any DHCP client request with the specified vendor ID (DHCP option 60) will be denied an IP address from the local DHCP server.
> 3.Select interfaces from the available interface list and add it to the grouped interface list using the arrow buttons to create the required mapping of the ports. Note that these clients may obtain public IP addresses
> 4. Click Apply/Save button to make the changes effective immediately
> IMPORTANT If a vendor ID is configured for a specific client device, please REBOOT the client device attached to the modem to allow it to obtain an appropriate IP address.
> Group Name:

> WAN Interface used in the grouping |

> Grouped LAN Interfaces |  | Available LAN Interfaces

> Automatically Add Clients With the following DHCP Vendor IDs