> System Log -- Configuration
> If the log mode is enabled, the system will begin to log all the selected events. For the Log Level, all events above or equal to the selected level will be logged. For the Display Level, all logged events above or equal to the selected level will be displayed. If the selected mode is 'Remote' or 'Both,' events will be sent to the specified IP address and UDP port of the remote syslog server. If the selected mode is 'Local' or 'Both,' events will be recorded in the local memory.
> Select the desired values and click 'Apply/Save' to configure the system log options.

> Log: | Disable | Enable

> Log Level: |
> Display Level: |
> Mode: |

> Server IP Address: |
> Server UDP Port: |