> NAT -- Virtual Servers Setup
> Virtual Server allows you to direct incoming traffic from the WAN interface (identified by its Protocol and External port) to the Internal server with a private IP address on the LAN interface. The Internal port is required only if the external port needs to be converted to a different port number used by the server on the LAN side. A maximum of 64 entries can be configured.
> Note: An IPv4 address is not editable if the IPv4 NAT function is turned off.
> Note: An IPv6 address is not editable if the IPv6 function of the interface is turned off.

> Server Name | External Port Start | External Port End | Protocol | Internal Port Start | Internal Port End | Server IPv4 Address | Server IPv6 Address | WAN Interface | LAN Loopback | Remove
> Age of Empires II Expansion: The Conquerors | 47624 | 47624 | TCP | 47624 | 47624 | 192.168.20.3 |  | All Interfaces | Disable |
> Age of Empires II Expansion: The Conquerors | 6073 | 6073 | TCP | 6073 | 6073 | 192.168.20.3 |  | All Interfaces | Disable |
> Age of Empires II Expansion: The Conquerors | 2300 | 2400 | TCP | 2300 | 2400 | 192.168.20.3 |  | All Interfaces | Disable |
> Age of Empires II Expansion: The Conquerors | 2300 | 2400 | UDP | 2300 | 2400 | 192.168.20.3 |  | All Interfaces | Disable |