> Interface Grouping -- A maximum 16 entries can be configured
> Interface Grouping supports multiple ports to WAN and bridging groups. Each group will perform as an independent network. To support this feature, you must create mapping groups with appropriate LAN and WAN interfaces using the Add button. The Remove button will remove the grouping and add the ungrouped interfaces to the Default group. Only the default group has IP interface.

> Group Name | Remove | WAN Interface | LAN Interfaces | DHCP Vendor IDs
> Default |