- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## SIP Settings

### Phone

- SIP Settings

### Fax Setting

Fax Negotiate Mode:
Bypass Codec:
Enable T38 redundancy support
Enable vbd redundancy support

### Settings

Enable VAD support
VAD mode in signal:
Enable RTCP Flow Ctrol
Enable Echo Cancellation
Enable # To ASCII

### SIP Timer Setting

Registration Expire Timeout:
Session Expire Timeout:
Min Session Expire Time: (need >= 90s)

### Digitmap Setting

Voip Dialpan Setting:

### Qos Setting

DSCP for SIP:
DSCP for RTP:
Ethernet Priority Mark:

### PayLoad Setting

RFC2198 Payload Value: (range 97~127)
Dtmf Relay setting:

### Call ID Setting

Caller ID send Delay Time: (range 500~1500ms)
Caller ID Message Type:
FSK modulation Mode:

### Transport Setting

SIP Transport protocol:

### SIP Extends

PRACK (100rel):

### Service Offer Setting

Complementary business models: