- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## IP Tunnel Configuration

### IPv4inIPv6 Tunnel Configuration

Name | WAN | LAN | Dynamic | AFTR | Remove
--- | --- | --- | --- | --- | ---

Add

## Add IPv4inIPv6 Tunnel

Currently, only DS-Lite configuration is supported.

Tunnel Name:
Mechanism:
Associated WAN Interface:
Associated LAN Interface:
Manual Automatic
AFTR:
Close

### IPv6inIPv4 Tunnel Configuration

Name | WAN | LAN | Dynamic | IPv4 Mask Length | 6rd Prefix | Border Relay Address | Remove
--- | --- | --- | --- | --- | --- | --- | ---

Add

## Add IPv6inIPv4 Tunnel

Currently, only 6rd configuration is supported.

Tunnel Name:
Mechanism:
Associated WAN Interface:
Associated LAN Interface:
Manual Automatic
IPv4 Mask Length:
6rd Prefix with Prefix Length:
Border Relay IPv4 Address:
Close