- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## Local Area Network

### Local Network

- LAN
- Wireless

IPV4 IPV6 VLAN

### IPv4 LAN Auto Configuration

Configure the Broadband Router IP Address and Subnet Mask for LAN interface.

IP Address:
Subnet Mask:
Enable IGMP Snooping
Enable DHCP Server Relay
DHCP Server IP Address

### DHCP

DHCP: On Off
DHCP Start Range:
DHCP End Range:
Primary DNS Server:
Secondary DNS Server:
DHCP Lease Time (Hour):

#### Static IP Lease list:

(A maximum 32 entries can be configured)

MAC Address | IP Address | Delete
--- | --- | ---

Add Entries

## DHCP Static IP Lease

Enter the Mac address and Static IP address then click "Apply/Save".

MAC Address:
IP Address:
Close
Enable IGMP LAN to LAN Multicast:

(LAN to LAN Multicast is enabled until the first WAN service is connected, regardless of the setting.)

#### DHCP Option Setup:

Code (1-254) | Value (255) | Address Pool | Enabled | Delete
--- | --- | --- | --- | ---

Add

## DHCP Option Setup

State: Enable Disable
Code: (1-254)
Value: (max length:255)
Pool:
Close

#### DHCP Option 60 Setup:

Device Class Name | Vendor ID | Vendor ID Match Mode | IP Address Start | IP Address End | Primary DNS | Secondary DNS | Gateway | DHCP Lease Time (seconds) | Enabled | Delete
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---

Add

## DHCP Option 60

State: Enable Disable
Device Class Name:
Vendor ID:
VendorId Match Mode: Exact Prefix Suffix Substring
IP Address Start:
IP Address End:
Primary DNS:
Secondary DNS:
Subnet Mask:
Gateway:
DHCP Lease Time(seconds):
Close

#### DHCP Port Setup

Enable or Disable DHCP for every interface.

You must enable lan ports.

eth0
eth1
eth2
eth3
wl0
wl0.1
wl0.2
wl0.3
wl1
wl1.1
wl1.2
wl1.3

### IPv6 LAN Auto Configuration

1: Stateful DHCPv6 is supported based on the assumption of prefix length less than 64. Interface ID does NOT support ZERO COMPRESSION "::". Please enter the complete information. For exampe: Please enter "0:0:0:2" instead of "::2".

2: Unique local address must start with "fd". The prefix and the address must be in same network and the prefix lenght must be 64.

ULA Prefix Advertisement: On Off

#### IPv6 LAN Applications

DHCP: On Off
Auto-Configuration: Stateless Stateful
Start Interface ID:
End Interface ID:
Leased Time (Hour):
RADVD: On Off
MLD: On Off
Standard Mode Blocking Mode
Enable MLD LAN to LAN Multicast: Enable Disable
DHCPV6 Relay Enable Disable
DHCPv6 Server IP Address:
Selected WAN Interface:
Hop limit:

### VLAN Setup

Select a LAN port:
Enable VLAN Mode

VLAN ID | Pbits | Delete
--- | --- | ---

Add

## VLAN

VLAN ID:
Pbits:
Close