- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## Troubleshooting

### Diagnostics

- Information
- Statistics
- Troubleshooting
- Logs

Your modem is capable of testing your DSL connection. The individual tests are listed below. If a test displays a fail status, click "Test" again to make sure the fail status is consistent. If the test continues to fail, click "Help" and follow the troubleshooting procedures

Test the connection to your local network

Test your eth0 Connection: | Pass | Help
Test your eth1 Connection: | Pass | Help
Test your eth2 Connection: | Fail | Help
Test your eth3 Connection: | Fail | Help
Test your eth4 Connection: | Pass | Help
Test your Wireless Connection: | Pass | Help

Test the connection to your DSL service provider

Test xDSL Synchronization: | Pass | Help
Test ATM OAM F5 segment ping: | Disabled | Help
Test ATM OAM F5 end-to-end ping: | Disabled | Help

Test the connection to your Internet service provider

Test PPP server connection: | Pass | Help
Test authentication with ISP: | Fail | Help
Test the assigned IP address: | Fail | Help
Ping default gateway: | Pass | Help
Ping primary Domain Name Server: | Pass | Help

### Ethernet OAM

#### Ethernet Link OAM (802.3ah)

Enable

#### Ethernet Service OAM (802.1ag / Y.1731)

Enable
802.1ag Y.1731

### Ping Diagnostic

Please type in a host name or an IP Address. Click Submit to check the connection automatically.

Host Name or Ip Address:

## Ping Diagnostic

This page shows the result of user's ping diagnostic test and connection test.

Test results PING 4.2.2.2 (4.2.2.2): 64 data bytes 72 bytes from 4.2.2.2: seq=0 ttl=53 time=150.718 ms 72 bytes from 4.2.2.2: seq=1 ttl=53 time=149.722 ms 72 bytes from 4.2.2.2: seq=2 ttl=53 time=149.421 ms 72 bytes from 4.2.2.2: seq=3 ttl=53 time=150.292 ms --- 4.2.2.2 ping statistics --- 4 packets transmitted, 4 packets received, 0 packet loss round-trip min/avg/max = 149.421/150.038/150.718 ms Close

### Traceroute Diagnostic

Please type in a host name or an IP Address. Click Submit to trace the route.

Host Name or Ip Address:

## Traceroute Diagnostic

This page shows user the route over the network between two systems, listing all the intermediate routers a connection must pass through to get to its destination.

Test results traceroute to 8.8.8.8 (8.8.8.8), 30 hops max, 38 byte packets 1 60.234.8.56 (60.234.8.56) 13.696 ms 13.210 ms 13.588 ms 2 72.14.243.237 (72.14.243.237) 36.425 ms 36.593 ms 36.318 ms 3 218.100.52.3 (218.100.52.3) 36.374 ms 36.678 ms 36.570 ms 4 108.170.247.65 (108.170.247.65) 37.003 ms 108.170.247.49 (108.170.247.49) 37.731 ms 37.122 ms 5 216.239.59.225 (216.239.59.225) 36.441 ms 216.239.41.79 (216.239.41.79) 37.083 ms 216.239.41.1 (216.239.41.1) 38.293 ms 6 8.8.8.8 (8.8.8.8) 36.802 ms 38.704 ms 36.663 ms Close

### Start/Stop DSL

This page enables you to start or stop your DSL line.

Your DSL connection is up.