- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## Routing

- NAT
- Routing
- DDNS

### Static Route

A maximum 32 entries can be configured.

IP Version | Destination IP/Mask | Gateway | Interface | Metric | Delete
--- | --- | --- | --- | --- | ---

Add

## Add Static Route

Enter the destination network address, subnet mask, gateway AND/OR available WAN interface then click "Apply/Save" to add the entry to the routing table.

IP Version: IPv4 IPv6
Destination IP address/prefix length:
Gateway:
Interface:
Metric: (optional: metric number should be greater than or equal to zero)
Close

### RIP Configuration

Note: RIP cannot be configured on the WAN interface which has NAT enabled (such as PPPoE).

To activate RIP for the WAN Interface, select the desired RIP version and operation and place a check in the "Enabled" checkbox. To stop RIP interface, uncheck the "Enabled" checkbox. Click "Apply/Save" button to Start/Stop RIP and save the configuration.

Interface | Version | Operation | Enabled
--- | --- | --- | ---
eth4.1 |  |  |

Apply/Save