- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## Wireless Advanced Settings

### Local Network

- LAN
- Wireless

Wireless Bridge MAC Filter Advanced

### Wireless Bridge

2.4 GHz 5 GHz

This page allows you to configure wireless bridge features of the wireless LAN interface. Select Disabled in Bridge Restrict which disables wireless bridge restriction. Any wireless bridge will be granted access. Selecting Enabled or Enabled(Scan) enables wireless bridge restriction. Only those bridges selected in Remote Bridges will be granted access.

Click "Refresh" to update the remote bridges. Wait for few seconds to update.

Click "Apply/Save" to configure the wireless bridge options.

AP Mode:
Bridge Restrict:
Remote Bridges MAC Address:

Remote Bridges MAC Address:

| SSID | BSSID
--- | --- | ---

This page allows you to configure wireless bridge features of the wireless LAN interface. Select Disabled in Bridge Restrict which disables wireless bridge restriction. Any wireless bridge will be granted access. Selecting Enabled or Enabled(Scan) enables wireless bridge restriction. Only those bridges selected in Remote Bridges will be granted access.

Click "Refresh" to update the remote bridges. Wait for few seconds to update.

Click "Apply/Save" to configure the wireless bridge options.

AP Mode:
Bridge Restrict:
Remote Bridges MAC Address:

Remote Bridges MAC Address:

| SSID | BSSID
--- | --- | ---

### MAC Filter

2.4 GHz 5 GHz
Select SSID:
MAC Restrict Mode: Disabled Allow Deny

MAC Address | Remove
--- | ---
AD:37:43:4F:A1:D4 | Delete

Add

## Add Network Traffic Class Rule

Enter the MAC address and click 'Apply/Save' to add the MAC address to the wireless MAC address filters.

MAC Address:
Close
Select SSID:
MAC Restrict Mode: Disabled Allow Deny

MAC Address | Remove
--- | ---
AD:37:43:4F:A1:D4 | Delete

Add

## Add Network Traffic Class Rule

Enter the MAC address and click 'Apply/Save' to add the MAC address to the wireless MAC address filters.

MAC Address:
Close

### Advanced

2.4 GHz 5 GHz

This page allws you to configure advanced features of the wireless LAN interface. You can select a particular channel on which to operate, force the transmission rate to a particular speed, set the fragmentation threshold, set the RTS threshold, set the wakeup interval for clients in power-save mode, set the beacon interval for the access point, set XPress mode and set whether short or long preambles are used.

Click 'Apply/Save' to configure the advanced wireless options.

Channel:
Current: 1 (interference: acceptable)
Auto Channel Timer(min):
802.11n/EWC:
Bandwidth:
Current: 40MHz
Control Sideband:
Current: Lower
802.11n Rate:
802.11n Protection:
Support 802.11n Client Only:
RIFS Advertisement:
OBSS Co-Existance:
RX Chain Power Save:
Power Save status: Low Power
RX Chain Power Save Quiet Time:
RX Chain Power Save PPS:
54g Rate:
Multicast Rate:
Basic Rate:
Fragmentation Threshold:
RTS Threshold:
DTIM Interval:
Beacon Interval:
Global Max Clients:
XPress Technology:
Transmit Power:
WMM(Wi-Fi Multimedia):
WMM No Acknowledgement:
WMM APSD:
Beamforming Transmission (BFR):
Beamforming Reception (BFE):
Band Steering:
Enable Traffic Scheduler:
Airtime Fairness:

This page allws you to configure advanced features of the wireless LAN interface. You can select a particular channel on which to operate, force the transmission rate to a particular speed, set the fragmentation threshold, set the RTS threshold, set the wakeup interval for clients in power-save mode, set the beacon interval for the access point, set XPress mode and set whether short or long preambles are used.

Click 'Apply/Save' to configure the advanced wireless options.

Channel:
Current: 1 (interference: acceptable)
Auto Channel Timer(min):
802.11n/EWC:
Bandwidth:
Current: 80MHz
Control Sideband:
Current: Lower
802.11n Rate:
802.11n Protection:
Support 802.11n Client Only:
RIFS Advertisement:
OBSS Co-Existance:
RX Chain Power Save:
Power Save status: Low Power
RX Chain Power Save Quiet Time:
RX Chain Power Save PPS:
54g Rate:
Multicast Rate:
Basic Rate:
Fragmentation Threshold:
RTS Threshold:
DTIM Interval:
Beacon Interval:
Global Max Clients:
XPress Technology:
Regulatory Mode:
Pre-Network Radar Check:
In-Network Radar Check:
TPC Mitigation(db):
Transmit Power:
WMM(Wi-Fi Multimedia):
WMM No Acknowledgement:
WMM APSD:
Beamforming Transmission (BFR):
Beamforming Reception (BFE):
Band Steering:
Enable Traffic Scheduler:
Airtime Fairness: