- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## MAC Filtering

### Security

- IP Filtering
- MAC Filtering
- IPSec
- Access Control

MAC Filtering is only effective on ATM PVCs configured in Bridge mode. FORWARDED means that all MAC layer frames will be FORWARDED except those matching with any of the specified rules in the following table. BLOCKED means that all MAC layer frames will be BLOCKED except those matching with any of the specified rules in the following table.

MAC Filtering Policy For Each Interface(maxinum 32 entries):

WARNING: Changing from one policy to another of an interface will cause all defined rules for that interface to be REMOVED AUTOMATICALLY! You will need to create new rules for the new policy.

Interface | Policy | Change
--- | --- | ---

Change Policy

Choose Add or Delete to configure MAC filtering rules.

Interface | Protocol | Destination MAC | Source MAC | Frame Direction | Delete
--- | --- | --- | --- | --- | ---

Add

## Add MAC Filter

Create a filter to identify the MAC layer frames by specifying at least on condition below. If multiple conditions are specified, all of them will take effect. Click "Apply/Save" to save and activate the filter.

Protocol Type:
Destination MAC Address:
Source MAC Address:
Frame Direction:
WAN Interfaces
(Configured in Bridge mode only)
Close