- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## NAT

### Routing

- NAT
- Routing
- DDNS

### Port Forwarding

Port Forwarding allows you to direct incoming traffic from WAN side (identified by Protocol and External port) to the Internal server with private IP address on the LAN side. The Internal port is required only if the external port needs to be converted to a different port number used by the server on the LAN side. A maximum 32 entries can be configured.

Server Name | External Port Start | External Port End | Protocol | Internal Port Start | Internal Port End | Server IP Address | WAN Interface | LAN Loopback | Enable | Delete
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---

Add

## Add Virtual Servers

Select the service name, and enter the server IP address and click "Apply/Save" to forward IP packets for this service to the specified server.

NOTE: The "Internal Port End" cannot be modified directly. Normally, it is set to the same value as "External Port End". However, if you modify "Internal Port Start", then "Internal Port End" will be set to the same value as "Internal Port Start".

Remaining number of entries that can be configured: 32

Use Interface:
Service Name:
LAN Loopback:
Server IP address:
Status:
External Port Start:
External Port End:
Protocol
Internal Port Start:
Internal Port End:
Close

### DMZ Host

The Broadband Router will forward IP packets from the WAN that do not belong to any of the applications configured in the Virtual Servers table to the DMZ host computer.

Enter the computer's IP address and click 'Apply' to activate the DMZ host.

Clear the IP address field and click 'Apply' to deactivate the DMZ host.

DMZ Host IP Address:
Enable LAN Loopback

### ALG

Select the ALG below.

FTP Enable
SIP Enable
TFTP Enable
H323 Enable
IRC Enable
Port Triggering Enable
PPTP Enable
IPSec Enable
RTSP Enable
SNMP Enable