- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## Port Shaping

### QoS

- Basic
- Queue
- Classification
- Port Shaping

QoS port shaping supports traffic shaping of Ethernet interface.

If "Shaping Rate" is set to "-1", it means no shaping and "Burst Size" will be ignored.

Interface | Type | Shaping Rate (Kbps) | Burst Size (bytes)
--- | --- | --- | ---
eth4 | WAN |  |
LAN1 | LAN |  |
LAN2 | LAN |  |
LAN3 | LAN |  |
LAN4 | LAN |  |