> ### Wireless Connection Test

> Pass: | Indicates that the Wireless interface from your computer is connected to the LAN port of your Broadband Router. A flashing or solid green LAN LED on the router also signifies that an Wireless connection is present and that this test is successful.
> Down: | Indicates that the Broadband Router does not detect the Wireless interface on your computer.

> If the test fails, follow the troubleshooting procedures listed below and rerun the diagnostics tests by clicking on the Rerun Diagnostic Tests button at the bottom of this page. If all the tests pass, close and restart your Web browser to access the Internet.

> Troubleshooting:

> 1. Verify that the Wireless configurations from your computer and your Broadband Router are matched and corrected.

> 2. Turn off the Broadband Router, wait 10 seconds and turn it back ON.

> 3. With the router on, press the reset button on the Broadband Router for at least five seconds and release it. This resets the Broadband Router to its default settings. Wait for the Broadband Router to initialize, then close and restart your Web browser. To reconfigure the router, type your DSL Account username and password.

> Contact ISP Technical Support if you have tried all of the above and still are experiencing a fail condition.