> WAN Setup - Summary
> Make sure that the settings below match the settings provided by your ISP.

> Connection Type: | L2TP
> NAT: | Disabled
> Full Cone NAT: | Disabled
> Firewall: | Disabled
> IGMP Multicast Proxy: | Disabled
> IGMP Multicast Source Enabled: | Disabled
> MLD Multicast Proxy: | Disabled
> MLD Multicast Source Enabled: | Disabled
> Quality Of Service: | Disabled

> L2TP Client Setup - Summary
> Make sure that the settings below match the settings provided by your ISP.

> VPN Type: | L2TP
> Server IP/Domain: | 1
> Authentication: | AUTO_AUTH
> MPPE: | Disabled
> MTU: | 1454
> NAT: | Disabled
> Firewall: | Disabled
> Enable: | Enabled

> Make sure that the settings below match the settings provided by your ISP.

> VPN Type: | PPTP
> Server IP: |
> Authentication: | AUTO_AUTH
> MPPE: | Disabled
> MTU: | 0
> NAT: | Disabled
> Firewall: | Disabled
> Enable: | Disabled

> Click "Apply/Save" to have this interface to be effective. Click "Back" to make any modifications.