> QoS Queue Setup
> In ATM mode, maximum 16 queues can be configured.
> In PTM mode, maximum 8 queues can be configured.
> For each Ethernet interface, maximum 4 queues can be configured.
> For each Ethernet WAN interface, maximum 4 queues can be configured.
> To add a queue, click the Add button.
> To remove queues, check their remove-checkboxes, then click the Remove button.
> The Enable button will scan through every queues in the table. Queues with enable-checkbox checked will be enabled. Queues with enable-checkbox un-checked will be disabled.
> The enable-checkbox also shows status of the queue after page reload.
> Note: Ethernet LAN queue configuration only takes effect when all the queues of the interface have been configured.

> Name | Key | Interface | Qid | Prec/Alg/Wght | DSL Latency | PTM Priority | Shaping Rate(bps) | Min Bit Rate(bps) | Burst Size(bytes) | Enable | Remove
> Default Queue | 33 | atm0 | 1 | 8/WRR/1 | Path0 |  |  |  |  |  |