> NAT -- Virtual Servers
> Select the service name, and enter the server IP address and click "Apply/Save" to forward IP packets for this service to the specified server.
> NOTE: The "Internal Port End" cannot be modified directly. Normally, it is set to the same value as "External Port End". However, if you modify "Internal Port Start", then "Internal Port End" will be set to the same value as "Internal Port Start".

> Remaining number of entries that can be configured: | 32

> Use Interface |
> Service Name:
> Select a Service: |
> Custom Service: |

> | Enable LAN Loopback

> Server IP Address: |

> Status: |

> External Port Start | External Port End | Protocol | Internal Port Start | Internal Port End