> QoS Classification Setup -- maximum 32 rules can be configured.
> To add a rule, click the Add button.
> To remove rules, check their remove-checkboxes, then click the Remove button.
> The Enable button will scan through every rules in the table. Rules with enable-checkbox checked will be enabled. Rules with enable-checkbox un-checked will be disabled.
> The enable-checkbox also shows status of the rule after page reload.
> If you disable WMM function in Wireless Page, classification related to wireless will not take effects

> | CLASSIFICATION CRITERIA |  |
> Class Name | Order | Class Interface | Ethernet Type | Source MAC/ Mask | Destination MAC/ Mask | Source IP/ Prefix Length | Destination | Min:Max/ IpLength | Protocol | Source Port | Destination | DSCP Check | 802.1P Check | TC Check | Queue Key | DSCP Mark | 802.1P Mark | TC Mark | Rate Limit(kbps) | Enable | Remove