> WAN Service Interface Configuration

> Select a layer 2 interface for this service

> Note: For ATM interface, the descriptor string is (portId_vpi_vci)
> For PTM interface, the descriptor string is (portId_high_low)
> Where portId=0 --> DSL Latency PATH0
> portId=1 --> DSL Latency PATH1
> portId=4 --> DSL Latency PATH0&1
> low =0 --> Low PTM Priority not set
> low =1 --> Low PTM Priority set
> high =0 --> High PTM Priority not set
> high =1 --> High PTM Priority set