> Basic > Quick Setup > Ethernet WAN only > IPoE Information
> You can configure your IP over Ethernet(IPoE) settings as supplied by your Internet Service Provider(ISP).
> if your ISP supplied a static IP address, you can enter the details here.
> Otherwise,select"Obtain an IP address automatically".

> | Obtain an IP address automatically
> | Use the following Static IP address
> | Allow multicast traffic without valid ip addresses

> | Option 55 Request List : |  | (e.g:1,3,6,12)
> | Option 58 Renewal Time: |  | (hour)
> | Option 59 Rebinding Time: |  | (hour)
> | Option 60 Vendor ID: |  |
> | Option 61 IAID: |  | (8 hexadecimal digits)
> | Option 61 DUID: |  | (hexadecimal digit)
> | Option 125: | Disable | Enable

> | WAN IP Address: |
> | WAN Subnet Mask: |
> | WAN gateway IP Address: |
> | Primary DNS server: |
> | Secondary DNS server: |

> | Enable IPv6 for this service

> | Obtain an IPv6 address automatically
> | Use the following Static IPv6 address

> | Request IPv6 Address
> | Request Prefix Delegation

> | WAN IPv6 Address: |
> | WAN IPv6 Prefix: |
> | WAN gateway IPv6 Address: |
> | PD: |
> | IPv6 Primary DNS server: |
> | IPv6 Secondary DNS server: |