> Statistics -- xDSL

> Synchronized Time: |
> Number of Synchronizations: | 0
> Mode: |
> Traffic Type: |
> Status: | Disabled
> Link Power State: |
> | Downstream | Upstream
> Line Coding(Trellis): |  |
> SNR Margin (0.1 dB): |  |
> Attenuation (0.1 dB): |  |
> Output Power (0.1 dBm): |  |
> Attainable Rate (Kbps): |  |
> Rate (Kbps): |  |
> Super Frames: |  |
> Super Frame Errors: |  |
> RS Words: |  |
> RS Correctable Errors: |  |
> RS Uncorrectable Errors: |  |
> | HEC Errors: |  |
> OCD Errors: |  |
> LCD Errors: |  |
> Total Cells: |  |
> Data Cells: |  |
> Bit Errors: |  |
> Total ES: |  |
> Total SES: |  |
> Total UAS: |  |