> Add Network Traffic Class Rule
> This screen creates a traffic class rule to classify the ingress traffic into a priority queue and optionally mark the DSCP or Ethernet priority of the packet.
> Click 'Apply/Save' to save and activate the rule.

> Traffic Class Name: |
> Rule Order: |
> Rule Status: |

> Specify Classification Criteria (A blank criterion indicates it is not used for classification.)

> Ingress Interface: |

> Ether Type: |

> Ether Type: |

> Source MAC Address: |

> Source MAC Mask: |
> Destination MAC Address: |
> Destination MAC Mask: |

> Destination IP Address[/Mask]: |

> IP Length Check(Min:Max): |

> Protocol: |

> Protocol: |

> UDP/TCP Source Port (port or port:port): |
> UDP/TCP Destination Port (port or port:port): |

> 802.1p Priority Check: |

> Specify Classification Results (A blank value indicates no operation.)

> Specify Egress Interface (Required): |

> Specify Egress Queue (Required): |

> - Packets classified into a queue that exit through an interface for which the queue
> is not specified to exist, will instead egress to the default queue on the interface.

> Specify Class Policer: |

> Mark 802.1p priority: |

> - Class non-vlan packets egress to a non-vlan interface will be tagged with VID 0 and the class rule p-bits.
> - Class vlan packets egress to a non-vlan interface will have the packet p-bits re-marked by the class rule p-bits. No additional vlan tag is added.
> - Class non-vlan packets egress to a vlan interface will be tagged with the interface VID and the class rule p-bits.
> - Class vlan packets egress to a vlan interface will be additionally tagged with the packet VID, and the class rule p-bits.