> Network Address Translation Settings
> Network Address Translation (NAT) allows you to share one Wide Area Network (WAN) IP address for multiple computers on your Local Area Network (LAN).

> | Enable NAT

> | Enable Fullcone NAT

> ONLY IF REQUIRED -- DISABLES NETWORK ACCELERATION AND SOME SECURITY

> | Enable Firewall

> Port Control Protocol Mode

> PCP Server |

> IGMP Multicast

> | Enable IGMP Multicast Proxy

> | Enable IGMP Multicast Source

> | No Multicast VLAN Filter

> MLD Multicast

> | Enable MLD Multicast Proxy

> | Enable MLD Multicast Source