> Local Area Network (LAN) Setup
> Configure the Broadband Router IP Address and Subnet Mask for LAN interface. Group Name

> IP Address: |
> Subnet Mask: |

> Enable IGMP Snooping

> Standard Mode
> Blocking Mode
> Enable IGMP LAN to LAN Multicast: |
> (LAN to LAN Multicast is enabled until the first WAN service is connected, regardless of this setting.)

> Enable LAN side firewall

> Disable DHCP Server
> Enable DHCP Server
> Start IP Address: |
> End IP Address: |
> Primary DNS server: |
> Secondary DNS server: |
> Leased Time (hour): |

> Static IP Lease List: (A maximum 32 entries can be configured)

>   MAC Address | IP Address | Remove

> Enable DHCP Server Relay
> DHCP Server IP Address: |

> Configure the second IP Address and Subnet Mask for LAN interface

> IP Address: |
> Subnet Mask: |