- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## Access Control

### Security

- IP Filtering
- MAC Filtering
- IPSec
- Access Control

Services access control list (SCL) enable or disable the running services.

Services | LAN | LAN Port | WAN | Port
--- | --- | --- | --- | ---
HTTP | Enable |  | Enable |
TELNET | Enable |  | Enable |
SSH | Enable |  | Enable |
FTP | Enable |  | Enable |
TFTP | Enable |  | Enable |
ICMP | Enable |  | Enable |
SNMP | Enable |  | Enable |
SAMBA | Enable |  | Enable |

### Access List

The IP Address Access Control mode, if enabled, permits access to local management services from IP addresses contained in the Access Control List. If the Access Control mode is disabled, the system will not validate IP addresses for incoming packets. The services are the system applications listed in the Service Control List.

Access Control Mode: Enable Disable

IP Address | Subnet Mask | Delete
--- | --- | ---

Add

## Add IP Addresses

Enter the IP address of the management station permitted to access the local management services, and click "Apply/Save".

IP Address:
Subnet Mask:
Close