- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## Information

### Diagnostics

- Information
- Statistics
- Troubleshooting
- Logs

### Device Info

Manufacturer:NetComm Wireless
Product Class:NF18ACV
Serial Number:02101863AAFF
Build Timestamp:160112_1320
Software Version:NF18ACV-NC2-R6BXXX.EN
Bootloader (CFE) Version:1.0.38-116.174
DSL PHY and Driver Version:A2pv6F039p.d26h
VDSL PROFILE:No profile
Wireless Driver Version:7.14.89.3303
Voice Service Version:V1.0
Voice Service Version:0D 17H 30M 7S

This information reflects the current status of your WAN connection.

Line Rate - Upstream (Kbps):1120
Line Rate - Downstream (Kbps):23216
LAN IPv4 Address:192.168.20.1
Service connection type:ADSL
Default Gateway:10.88.158.1
Primary DNS Server:172.24.10.10
Secondary DNS Server:172.24.10.11
LAN IPv6 ULA Address:
Default IPv6 Gateway:

### WAN

Interface | Description | Type | VLAN Mux ID | IPv6 | IGMP Pxy | IGMP Src Enbl | MLD Pxy | MLD Src Enbl | NAT | Firewall | Status | IPv4 Address | IPv6 Address
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
ppp0.1 | ADSL | PPPoE | Disabled | Disabled | Disabled | Disabled |  |  | Enabled | Enabled | Connected | 10.88.158.172 |

### Route

Flags: U - up, ! - reject, G - gateway, H - host, R - reinstate, D - dynamic (redirect), M - modified (redirect).

Destination | Gateway | Subnet Mask | Flag | Metric | Service | Interface
--- | --- | --- | --- | --- | --- | ---
0.0.0.0 | 0.0.0.0 | 0.0.0.0 | U | 0 | ADSL | ppp0.1
10.88.158.1 | 0.0.0.0 | 255.255.255.255 | UH | 0 | ADSL | ppp0.1
192.168.20.0 | 0.0.0.0 | 255.255.255.0 | U | 0 |  | br0

### ARP

IP address | Flags | HW Address | Device
--- | --- | --- | ---
192.168.20.11 | Complete | 00:e0:4c:68:0a:ba | br0