- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## Diagnostics

- Information
- Statistics
- Performance
- Troubleshooting
- Logs

### Statistics - LAN

Interface | Received | Transmitted
--- | --- | ---
Total | Multicast | Unicast | Broadcast | Total | Multicast | Unicast | Broadcast
Bytes | Pkts | Errs | Drops | Bytes | Pkts | Pkts | Pkts | Bytes | Pkts | Errs | Drops | Bytes | Pkts | Pkts | Pkts
eth0 | 2030875 | 20161 | 0 | 0 | 0 | 3873 | 15231 | 1057 | 16832258 | 32635 | 0 | 0 | 0 | 12820 | 19805 | 10
eth1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
eth2 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
eth3 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
eth4 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 1471168 | 16448 | 0 | 0 | 0 | 15387 | 0 | 1061
wl0 | 0 | 0 | 0 | 11 | 0 | 0 | 0 | 0 | 1510348 | 16309 | 0 | 0 | 0 | 15315 | 0 | 1017
wl0.1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
wl0.2 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0
wl0.3 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0

### Statistics - WAN Service

Interface | Description | Received | Transmitted
--- | --- | --- | ---
Total | Multicast | Unicast | Broadcast | Total | Multicast | Unicast | Broadcast
Bytes | Pkts | Errs | Drops | Bytes | Pkts | Pkts | Pkts | Bytes | Pkts | Errs | Drops | Bytes | Pkts | Pkts | Pkts
ppp0.1 | ADSL | 54 | 3 | 0 | 0 | 0 | 0 | 3 | 0 | 930 | 6 | 0 | 0 | 0 | 0 | 6 | 0

### Statistics - xTM

Port Number | In Octets | Out Octets | In Packets | Out Packets | In OAM Cells | Out OAM Cells | In ASM Cells | Out ASM Cells | In Packet Errors | In Cell Errors
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
1 | 1830037 | 43407 | 701 | 400 | 0 | 0 | 0 | 0 | 0 | 32287

### Statistics - xDSL

Mode: | ADSL_2plus
Traffic Type: | ATM
Status: | Up
Link Power State: | L0
| Downstream | Upstream
--- | --- | ---
Line Coding(Trellis): | On | On
SNR Margin (0.1 dB): | 83 | 80
Attenuation (0.1 dB): | 35 | 19
Output Power (0.1 dBm): | 192 | 26
Attainable Rate (Kbps): | 24360 | 1240
| Path 0 | Path 1
| Downstream | Upstream | Downstream | Upstream
Rate (Kbps): | 23216 | 1120 | 0 | 0
MSGc (# of bytes in overhead channel message): | 58 | 84 | 0 | 0
B (# of bytes in Mux Data Frame): | 242 | 28 | 0 | 0
M (# of Mux Data Frames in FEC Data Frame): | 1 | 8 | 0 | 0
T (Mux Data Frames over sync bytes): | 3 | 1 | 0 | 0
R (# of check bytes in FEC Data Frame): | 12 | 16 | 0 | 0
S (ratio of FEC over PMD Data Frame length): | 0.3344 | 6.4000 | 0.0000 | 0.0000
L (# of bits in PMD Data Frame): | 6099 | 310 | 0 | 0
D (interleaver depth): | 64 | 8 | 0 | 0
Delay (msec): | 5 | 13 | 0 | 0
INP (DMT symbol): | 0.50 | 1.50 | 0.00 | 0.00
Super Frames: | 367399 | 326234 | 0 | 0
Super Frame Errors: | 0 | 46 | 0 | 0
RS Words: | 70540376 | 3687515 | 0 | 0
RS Correctable Errors: | 41 | 5012 | 0 | 0
RS Uncorrectable Errors: | 29 | 0 | 0 | 0
HEC Errors: | 5 | 40 | 0 | 0
OCD Errors: | 0 | 0 | 0 | 0
LCD Errors: | 0 | 0 | 0 | 0
Total Cells: | 322978965 | 15536241 | 0 | 0
Data Cells: | 32865 | 731 | 0 | 0
Bit Errors: | 1337 | 0 | 0 | 0
Total ES: | 1 | 34
Total SES: | 0 | 0
Total UAS: | 62916 | 62916