> Basic > Quick Setup > Internet Setup

> This Wizard is designed to walk you through the basic information needed to set up your device

> To continue, please select your WAN connection type.

> ADSL

> VDSL

> Ethernet WAN

> Basic > Quick Setup > WAN Setup (Select one WAN mode)

> Select the WAN mode for your internet connection as specified by your Internet Service Provider(ISP).

> PPP Over Ethernet (PPPoE)

> IP Over Ethernet (IPoE)

> Bridging

> PPP Over ATM (PPPoA)

> Basic > Quick Setup > VLAN Setup

> Please select the correct VLAN option for your connection:
> If you are unsure, please contact your ISP

> No VLAN Tag

> VLAN Tag 10(For most New Zealand Customers)

> Custom VLAN Tag

> VLAN Tag: |  | (0-4094)

> Basic > Quick Setup > PVC Setup

> Please enter the correct PVC number for your connection:
> If you are unsure, please contact your ISP

> VPI:

> VCI:

> Basic > Quick Setup > Ethernet WAN only > PPPoE Information

> Enter the User ID and Password assigned to you by your Internet Service Provider (ISP).

> User ID: |
> Password: |

> Basic > Quick Setup > Ethernet WAN only > IPoE Information
> You can configure your IP over Ethernet(IPoE) settings as supplied by your Internet Service Provider(ISP).
> if your ISP supplied a static IP address, you can enter the details here.
> Otherwise,select"Obtain an IP address automatically".

> | Obtain an IP address automatically
> | Use the following Static IP address

> | WAN IP Address: |
> | WAN Subnet Mask: |
> | WAN gateway IP Address: |
> | Primary DNS server: |
> | Secondary DNS server: |

> WAN Basic Setup - Summary
> Make sure that the settings below match the settings provided by your ISP.

> Connection Type: | PPPoE
> NAT: | Enabled
> Full Cone NAT: | Disabled
> Firewall: | Enabled
> IGMP Multicast Proxy: | Disabled
> IGMP Multicast Source Enabled: | Disabled
> MLD Multicast Proxy: | Disabled
> MLD Multicast Source Enabled: | Disabled
> Quality Of Service: | Enabled

> Click "Apply/Save" to have this interface to be effective. Click "Back" to make any modifications.