> Multicast Precedence: | lower value, higher priority
> Multicast Strict Grouping Enforcement: |

> Enable Multicast DSCP Remarking
> Multicast DSCP Remarking: |

> IGMP Configuration
> Enter IGMP protocol configuration fields if you want modify default values shown below.

> Default Version: |
> Query Interval (s): |
> Query Response Interval (1/10s): |
> Robustness Interval (1/10s): |
> Robustness Value: |
> Maximum Multicast Groups: |
> Maximum Multicast Data Sources (for IGMPv3): |
> Maximum Multicast Group Members: |
> Fast Leave Enable: |

> IGMP Group Exception List

> Group Address | Mask/Mask bits | Remove
> 224.0.0.0 | 255.255.255.0 |

> MLD Configuration
> Enter MLD protocol (IPv6 Multicast) configuration fields if you want modify default values shown below.

> Default Version: |
> Query Interval (s): |
> Query Response Interval (1/10s): |
> Robustness Interval (1/10s): |
> Robustness Value: |
> Maximum Multicast Groups: |
> Maximum Multicast Data Sources (for mldv2): |
> Maximum Multicast Group Members: |
> Fast Leave Enable: |

> MLD Group Exception List

> Group Address | Mask/Mask bits | Remove
> ff01::0000 | ffff::0000 |
> ff02::0000 | ffff::0000 |